PASSED MOTION FOR "WOOD FENCE" REPLACEMENT

Effective May 10th, 2017, the board shall consider and may approve required variance request(s) for wood fence replacement under the following guidelines. These guidelines are for wood material fencing only. All aspects that comprise wood material fences are inclusive for all parts and components.
1)	All fence material, which includes boards, slats, braces, gates and posts, must be constructed of pressure treated lumber.
2)	Fence height must be between 5 – 6 feet.  
3)	Gates are required and must be the same height as adjoining fence sections. 
4)	Door hinges and door handle must be black in color.
5)	Fence posts must be securely buried and reinforced as required.
6)	Variations in fence height will be allowed due to any uneven landscape terrain, accommodating a uniform fence height, as documented on the Fence Variance Request.
7)	Fencing must consist of privacy fence panels as documented on the Variance Request.

5-9-2017